[    0.000000] kernel: Booting Linux on physical CPU 0x0000000000 [0x410fd034]
[    0.000000] kernel: Linux version 5.15.0-1005-raspi (buildd@bos02-arm64-056) (gcc (Ubuntu 11.2.0-19ubuntu1) 11.2.0, GNU ld (GNU Binutils for Ubuntu) 2.38) #5-Ubuntu SMP PREEMPT Mon Apr 4 12:21:48 UTC 2022 (Ubuntu 5.15.0-1005.5-raspi 5.15.30)
[    0.000000] kernel: random: fast init done
[    0.000000] kernel: Machine model: Raspberry Pi 3 Model B Rev 1.2
[    0.000000] kernel: efi: UEFI not found.
[    0.000000] kernel: Reserved memory: created CMA memory pool at 0x0000000037400000, size 64 MiB
[    0.000000] kernel: OF: reserved mem: initialized node linux,cma, compatible id shared-dma-pool
[    0.000000] kernel: Zone ranges:
[    0.000000] kernel:   DMA      [mem 0x0000000000000000-0x000000003b3fffff]
[    0.000000] kernel:   DMA32    empty
[    0.000000] kernel:   Normal   empty
[    0.000000] kernel: Movable zone start for each node
[    0.000000] kernel: Early memory node ranges
[    0.000000] kernel:   node   0: [mem 0x0000000000000000-0x000000003b3fffff]
[    0.000000] kernel: Initmem setup node 0 [mem 0x0000000000000000-0x000000003b3fffff]
[    0.000000] kernel: percpu: Embedded 29 pages/cpu s80344 r8192 d30248 u118784
[    0.000000] kernel: pcpu-alloc: s80344 r8192 d30248 u118784 alloc=29*4096
[    0.000000] kernel: pcpu-alloc: [0] 0 [0] 1 [0] 2 [0] 3 
[    0.000000] kernel: Detected VIPT I-cache on CPU0
[    0.000000] kernel: CPU features: kernel page table isolation forced ON by KASLR
[    0.000000] kernel: CPU features: detected: Kernel page table isolation (KPTI)
[    0.000000] kernel: CPU features: detected: ARM erratum 843419
[    0.000000] kernel: CPU features: detected: ARM erratum 845719
[    0.000000] kernel: Built 1 zonelists, mobility grouping on.  Total pages: 238896
[    0.000000] kernel: Kernel command line: coherent_pool=1M 8250.nr_uarts=1 snd_bcm2835.enable_compat_alsa=0 snd_bcm2835.enable_hdmi=1 bcm2708_fb.fbwidth=720 bcm2708_fb.fbheight=480 bcm2708_fb.fbswap=1 vc_mem.mem_base=0x3ec00000 vc_mem.mem_size=0x40000000  console=ttyS0,115200 dwc_otg.lpm_enable=0 console=tty1 root=LABEL=writable rootfstype=ext4 rootwait fixrtc quiet splash
[    0.000000] kernel: Unknown kernel command line parameters "fixrtc splash", will be passed to user space.
[    0.000000] kernel: Dentry cache hash table entries: 131072 (order: 8, 1048576 bytes, linear)
[    0.000000] kernel: Inode-cache hash table entries: 65536 (order: 7, 524288 bytes, linear)
[    0.000000] kernel: mem auto-init: stack:off, heap alloc:off, heap free:off
[    0.000000] kernel: Memory: 815224K/970752K available (14464K kernel code, 2672K rwdata, 5176K rodata, 5760K init, 876K bss, 89992K reserved, 65536K cma-reserved)
[    0.000000] kernel: random: get_random_u64 called from kmem_cache_open+0x34/0x334 with crng_init=1
[    0.000000] kernel: SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=4, Nodes=1
[    0.000000] kernel: ftrace: allocating 44049 entries in 173 pages
[    0.000000] kernel: ftrace: allocated 173 pages with 5 groups
[    0.000000] kernel: trace event string verifier disabled
[    0.000000] kernel: rcu: Preemptible hierarchical RCU implementation.
[    0.000000] kernel: rcu:         RCU restricting CPUs from NR_CPUS=256 to nr_cpu_ids=4.
[    0.000000] kernel:         Trampoline variant of Tasks RCU enabled.
[    0.000000] kernel:         Rude variant of Tasks RCU enabled.
[    0.000000] kernel:         Tracing variant of Tasks RCU enabled.
[    0.000000] kernel: rcu: RCU calculated value of scheduler-enlistment delay is 25 jiffies.
[    0.000000] kernel: rcu: Adjusting geometry for rcu_fanout_leaf=16, nr_cpu_ids=4
[    0.000000] kernel: NR_IRQS: 64, nr_irqs: 64, preallocated irqs: 0
[    0.000000] kernel: Root IRQ handler: bcm2836_arm_irqchip_handle_irq
[    0.000000] kernel: arch_timer: cp15 timer(s) running at 19.20MHz (phys).
[    0.000000] kernel: clocksource: arch_sys_counter: mask: 0xffffffffffffff max_cycles: 0x46d987e47, max_idle_ns: 440795202767 ns
[    0.000001] kernel: sched_clock: 56 bits at 19MHz, resolution 52ns, wraps every 4398046511078ns
[    0.000317] kernel: Console: colour dummy device 80x25
[    0.000392] kernel: printk: console [tty1] enabled
[    0.000467] kernel: Calibrating delay loop (skipped), value calculated using timer frequency.. 38.40 BogoMIPS (lpj=76800)
[    0.000507] kernel: pid_max: default: 32768 minimum: 301
[    0.000826] kernel: LSM: Security Framework initializing
[    0.000904] kernel: Yama: becoming mindful.
[    0.001093] kernel: AppArmor: AppArmor initialized
[    0.001335] kernel: Mount-cache hash table entries: 2048 (order: 2, 16384 bytes, linear)
[    0.001378] kernel: Mountpoint-cache hash table entries: 2048 (order: 2, 16384 bytes, linear)
[    0.006210] kernel: rcu: Hierarchical SRCU implementation.
[    0.008405] kernel: EFI services will not be available.
[    0.009793] kernel: smp: Bringing up secondary CPUs ...
[    0.011494] kernel: Detected VIPT I-cache on CPU1
[    0.011591] kernel: CPU1: Booted secondary processor 0x0000000001 [0x410fd034]
[    0.013603] kernel: Detected VIPT I-cache on CPU2
[    0.013677] kernel: CPU2: Booted secondary processor 0x0000000002 [0x410fd034]
[    0.015487] kernel: Detected VIPT I-cache on CPU3
[    0.015551] kernel: CPU3: Booted secondary processor 0x0000000003 [0x410fd034]
[    0.015778] kernel: smp: Brought up 1 node, 4 CPUs
[    0.015808] kernel: SMP: Total of 4 processors activated.
[    0.015825] kernel: CPU features: detected: 32-bit EL0 Support
[    0.015840] kernel: CPU features: detected: 32-bit EL1 Support
[    0.015859] kernel: CPU features: detected: CRC32 instructions
[    0.016270] kernel: CPU features: emulated: Privileged Access Never (PAN) using TTBR0_EL1 switching
[    0.053688] kernel: CPU: All CPU(s) started at EL2
[    0.053812] kernel: alternatives: patching kernel code
[    0.056333] kernel: devtmpfs: initialized
[    0.077000] kernel: Enabled cp15_barrier support
[    0.077051] kernel: Enabled setend support
[    0.077080] kernel: KASLR enabled
[    0.077396] kernel: clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 7645041785100000 ns
[    0.077440] kernel: futex hash table entries: 1024 (order: 4, 65536 bytes, linear)
[    0.081687] kernel: pinctrl core: initialized pinctrl subsystem
[    0.082842] kernel: DMI not present or invalid.
[    0.083848] kernel: NET: Registered PF_NETLINK/PF_ROUTE protocol family
[    0.094274] kernel: DMA: preallocated 1024 KiB GFP_KERNEL pool for atomic allocations
[    0.094784] kernel: DMA: preallocated 1024 KiB GFP_KERNEL|GFP_DMA pool for atomic allocations
[    0.096140] kernel: DMA: preallocated 1024 KiB GFP_KERNEL|GFP_DMA32 pool for atomic allocations
[    0.096251] kernel: audit: initializing netlink subsys (disabled)
[    0.096698] kernel: audit: type=2000 audit(0.096:1): state=initialized audit_enabled=0 res=1
[    0.097670] kernel: thermal_sys: Registered thermal governor 'fair_share'
[    0.097689] kernel: thermal_sys: Registered thermal governor 'bang_bang'
[    0.097707] kernel: thermal_sys: Registered thermal governor 'step_wise'
[    0.097723] kernel: thermal_sys: Registered thermal governor 'user_space'
[    0.098051] kernel: cpuidle: using governor ladder
[    0.098132] kernel: cpuidle: using governor menu
[    0.098752] kernel: hw-breakpoint: found 6 breakpoint and 4 watchpoint registers.
[    0.099032] kernel: ASID allocator initialised with 32768 entries
[    0.099411] kernel: Serial: AMBA PL011 UART driver
[    0.110417] kernel: bcm2835-mbox 3f00b880.mailbox: mailbox enabled
[    0.136721] kernel: raspberrypi-firmware soc:firmware: Attached to firmware from 2021-11-18T16:18:09, variant start
[    0.140744] kernel: raspberrypi-firmware soc:firmware: Firmware hash is d9b293558b4cef6aabedcc53c178e7604de90788
[    0.188237] kernel: HugeTLB registered 1.00 GiB page size, pre-allocated 0 pages
[    0.188275] kernel: HugeTLB registered 32.0 MiB page size, pre-allocated 0 pages
[    0.188295] kernel: HugeTLB registered 2.00 MiB page size, pre-allocated 0 pages
[    0.188314] kernel: HugeTLB registered 64.0 KiB page size, pre-allocated 0 pages
[    0.205598] kernel: bcm2835-dma 3f007000.dma: DMA legacy API manager, dmachans=0x1
[    0.211479] kernel: iommu: Default domain type: Translated 
[    0.211511] kernel: iommu: DMA domain TLB invalidation policy: strict mode 
[    0.213513] kernel: SCSI subsystem initialized
[    0.213934] kernel: libata version 3.00 loaded.
[    0.214245] kernel: usbcore: registered new interface driver usbfs
[    0.214323] kernel: usbcore: registered new interface driver hub
[    0.214410] kernel: usbcore: registered new device driver usb
[    0.214928] kernel: pps_core: LinuxPPS API ver. 1 registered
[    0.214947] kernel: pps_core: Software ver. 5.3.6 - Copyright 2005-2007 Rodolfo Giometti <giometti@linux.it>
[    0.214982] kernel: PTP clock support registered
[    0.215404] kernel: EDAC MC: Ver: 3.0.0
[    0.217974] kernel: NetLabel: Initializing
[    0.217996] kernel: NetLabel:  domain hash size = 128
[    0.218014] kernel: NetLabel:  protocols = UNLABELED CIPSOv4 CALIPSO
[    0.218158] kernel: NetLabel:  unlabeled traffic allowed by default
[    0.219690] kernel: clocksource: Switched to clocksource arch_sys_counter
[    0.347795] kernel: VFS: Disk quotas dquot_6.6.0
[    0.347941] kernel: VFS: Dquot-cache hash table entries: 512 (order 0, 4096 bytes)
[    0.349376] kernel: AppArmor: AppArmor Filesystem Enabled
[    0.364920] kernel: NET: Registered PF_INET protocol family
[    0.365223] kernel: IP idents hash table entries: 16384 (order: 5, 131072 bytes, linear)
[    0.367445] kernel: tcp_listen_portaddr_hash hash table entries: 512 (order: 1, 8192 bytes, linear)
[    0.367508] kernel: TCP established hash table entries: 8192 (order: 4, 65536 bytes, linear)
[    0.367637] kernel: TCP bind hash table entries: 8192 (order: 5, 131072 bytes, linear)
[    0.367889] kernel: TCP: Hash tables configured (established 8192 bind 8192)
[    0.368386] kernel: MPTCP token hash table entries: 1024 (order: 2, 24576 bytes, linear)
[    0.368491] kernel: UDP hash table entries: 512 (order: 2, 16384 bytes, linear)
[    0.368557] kernel: UDP-Lite hash table entries: 512 (order: 2, 16384 bytes, linear)
[    0.368950] kernel: NET: Registered PF_UNIX/PF_LOCAL protocol family
[    0.369001] kernel: NET: Registered PF_XDP protocol family
[    0.369029] kernel: PCI: CLS 0 bytes, default 64
[    0.369518] kernel: Trying to unpack rootfs image as initramfs...
[    0.381084] kernel: hw perfevents: enabled with armv8_cortex_a53 PMU driver, 7 counters available
[    0.381468] kernel: kvm [1]: IPA Size Limit: 40 bits
[    0.384103] kernel: kvm [1]: Hyp mode initialized successfully
[    0.389087] kernel: Initialise system trusted keyrings
[    0.389212] kernel: Key type blacklist registered
[    0.389693] kernel: workingset: timestamp_bits=46 max_order=18 bucket_order=0
[    0.401497] kernel: zbud: loaded
[    0.404462] kernel: squashfs: version 4.0 (2009/01/31) Phillip Lougher
[    0.405991] kernel: fuse: init (API version 7.34)
[    0.480069] kernel: Key type asymmetric registered
[    0.480115] kernel: Asymmetric key parser 'x509' registered
[    0.480328] kernel: Block layer SCSI generic (bsg) driver version 0.4 loaded (major 242)
[    0.480726] kernel: io scheduler mq-deadline registered
[    0.492325] kernel: bcm2708_fb soc:fb: FB found 1 display(s)
[    0.506087] kernel: Console: switching to colour frame buffer device 90x30
[    0.511371] kernel: bcm2708_fb soc:fb: Registered framebuffer for display 0, size 720x480
[    0.615754] kernel: Serial: 8250/16550 driver, 1 ports, IRQ sharing enabled
[    0.619625] kernel: bcm2835-rng 3f104000.rng: hwrng registered
[    0.620651] kernel: vc-mem: phys_addr:0x00000000 mem_base=0x3ec00000 mem_size:0x40000000(1024 MiB)
[    0.622375] kernel: cacheinfo: Unable to detect cache hierarchy for CPU 0
[    0.638525] kernel: loop: module loaded
[    0.646195] kernel: tun: Universal TUN/TAP device driver, 1.6
[    0.646879] kernel: PPP generic driver version 2.4.2
[    0.647315] kernel: usbcore: registered new interface driver lan78xx
[    0.647396] kernel: usbcore: registered new interface driver smsc95xx
[    0.647449] kernel: ehci_hcd: USB 2.0 'Enhanced' Host Controller (EHCI) Driver
[    0.647532] kernel: ehci-pci: EHCI PCI platform driver
[    0.647609] kernel: ohci_hcd: USB 1.1 'Open' Host Controller (OHCI) Driver
[    0.647642] kernel: ohci-pci: OHCI PCI platform driver
[    0.647779] kernel: uhci_hcd: USB Universal Host Controller Interface driver
[    0.647947] kernel: dwc_otg: version 3.00a 10-AUG-2012 (platform bus)
[    0.648263] kernel: dwc_otg: FIQ enabled
[    0.648280] kernel: dwc_otg: NAK holdoff enabled
[    0.648295] kernel: dwc_otg: FIQ split-transaction FSM enabled
[    0.648315] kernel: Module dwc_common_port init
[    0.649153] kernel: mousedev: PS/2 mouse device common for all mice
[    0.649814] kernel: i2c_dev: i2c /dev entries driver
[    0.653082] kernel: device-mapper: core: CONFIG_IMA_DISABLE_HTABLE is disabled. Duplicate IMA measurements will not be recorded in the IMA log.
[    0.653326] kernel: device-mapper: uevent: version 1.0.3
[    0.653809] kernel: device-mapper: ioctl: 4.45.0-ioctl (2021-03-22) initialised: dm-devel@redhat.com
[    0.657274] kernel: sdhci: Secure Digital Host Controller Interface driver
[    0.657305] kernel: sdhci: Copyright(c) Pierre Ossman
[    0.657924] kernel: sdhci-pltfm: SDHCI platform and OF driver helper
[    0.661816] kernel: ledtrig-cpu: registered to indicate activity on CPUs
[    0.662387] kernel: hid: raw HID events driver (C) Jiri Kosina
[    0.668030] kernel: drop_monitor: Initializing network drop monitor service
[    0.668778] kernel: NET: Registered PF_INET6 protocol family
[    1.126525] kernel: Freeing initrd memory: 40392K
[    1.168254] kernel: Segment Routing with IPv6
[    1.168365] kernel: In-situ OAM (IOAM) with IPv6
[    1.168452] kernel: NET: Registered PF_PACKET protocol family
[    1.168669] kernel: Key type dns_resolver registered
[    1.169718] kernel: registered taskstats version 1
[    1.169794] kernel: Loading compiled-in X.509 certificates
[    1.172912] kernel: Loaded X.509 cert 'Build time autogenerated kernel key: 78070d79cc76580dfaf75152e5a90b2b2efd68a2'
[    1.175555] kernel: Loaded X.509 cert 'Canonical Ltd. Live Patch Signing: 14df34d1a87cf37625abec039ef2bf521249b969'
[    1.178215] kernel: Loaded X.509 cert 'Canonical Ltd. Kernel Module Signing: 88f752e560a1e0737e31163a466ad7b70a850c19'
[    1.178229] kernel: blacklist: Loading compiled-in revocation X.509 certificates
[    1.178306] kernel: Loaded X.509 cert 'Canonical Ltd. Secure Boot Signing: 61482aa2830d0ab2ad5af10b7250da9033ddcef0'
[    1.178980] kernel: Key type ._fscrypt registered
[    1.178992] kernel: Key type .fscrypt registered
[    1.179001] kernel: Key type fscrypt-provisioning registered
[    1.208786] kernel: Key type encrypted registered
[    1.208823] kernel: AppArmor: AppArmor sha1 policy hashing enabled
[    1.208878] kernel: ima: No TPM chip found, activating TPM-bypass!
[    1.208924] kernel: ima: Allocated hash algorithm: sha1
[    1.208991] kernel: ima: No architecture policies found
[    1.209120] kernel: evm: Initialising EVM extended attributes:
[    1.209131] kernel: evm: security.selinux
[    1.209142] kernel: evm: security.SMACK64
[    1.209153] kernel: evm: security.SMACK64EXEC
[    1.209163] kernel: evm: security.SMACK64TRANSMUTE
[    1.209173] kernel: evm: security.SMACK64MMAP
[    1.209183] kernel: evm: security.apparmor
[    1.209193] kernel: evm: security.ima
[    1.209202] kernel: evm: security.capability
[    1.209212] kernel: evm: HMAC attrs: 0x1
[    1.219760] kernel: uart-pl011 3f201000.serial: cts_event_workaround enabled
[    1.219946] kernel: 3f201000.serial: ttyAMA0 at MMIO 0x3f201000 (irq = 99, base_baud = 0) is a PL011 rev2
[    1.223426] kernel: bcm2835-aux-uart 3f215040.serial: there is not valid maps for state default
[    1.225299] kernel: printk: console [ttyS0] disabled
[    1.225423] kernel: 3f215040.serial: ttyS0 at MMIO 0x3f215040 (irq = 71, base_baud = 50000000) is a 16550
[    1.225641] kernel: printk: console [ttyS0] enabled
[    1.227222] kernel: bcm2835-wdt bcm2835-wdt: Broadcom BCM2835 watchdog timer
[    1.227769] kernel: bcm2835-power bcm2835-power: Broadcom BCM2835 power domains driver
[    1.229485] kernel: mmc-bcm2835 3f300000.mmcnr: mmc_debug:0 mmc_debug2:0
[    1.229501] kernel: mmc-bcm2835 3f300000.mmcnr: DMA channel allocated
[    1.255228] kernel: sdhost: log_buf @ (____ptrval____) (c59a7000)
[    1.319769] kernel: mmc0: sdhost-bcm2835 loaded - DMA enabled (>1)
[    1.322662] kernel: of_cfs_init
[    1.322822] kernel: of_cfs_init: OK
[    1.334726] kernel: Freeing unused kernel memory: 5760K
[    1.355603] kernel: Checked W+X mappings: passed, no W+X pages found
[    1.355645] kernel: Run /init as init process
[    1.355670] kernel:   with arguments:
[    1.355680] kernel:     /init
[    1.355689] kernel:     fixrtc
[    1.355697] kernel:     splash
[    1.355705] kernel:   with environment:
[    1.355713] kernel:     HOME=/
[    1.355721] kernel:     TERM=linux
[    1.389030] kernel: mmc0: host does not support reading read-only switch, assuming write-enable
[    1.393128] kernel: mmc1: new high speed SDIO card at address 0001
[    1.394607] kernel: mmc0: new high speed SDXC card at address aaaa
[    1.395616] kernel: mmcblk0: mmc0:aaaa SN256 238 GiB 
[    1.398888] kernel:  mmcblk0: p1 p2
[    1.399510] kernel: mmcblk0: mmc0:aaaa SN256 238 GiB
[    2.407615] kernel: usb_phy_generic phy: supply vcc not found, using dummy regulator
[    3.034119] kernel: dwc2 3f980000.usb: supply vusb_d not found, using dummy regulator
[    3.034462] kernel: dwc2 3f980000.usb: supply vusb_a not found, using dummy regulator
[    3.243826] kernel: dwc2 3f980000.usb: EPs: 8, dedicated fifos, 4080 entries in SPRAM
[    3.244266] kernel: dwc2 3f980000.usb: DWC OTG Controller
[    3.244311] kernel: dwc2 3f980000.usb: new USB bus registered, assigned bus number 1
[    3.244374] kernel: dwc2 3f980000.usb: irq 51, io mem 0x3f980000
[    3.244896] kernel: usb usb1: New USB device found, idVendor=1d6b, idProduct=0002, bcdDevice= 5.15
[    3.244921] kernel: usb usb1: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    3.244942] kernel: usb usb1: Product: DWC OTG Controller
[    3.244959] kernel: usb usb1: Manufacturer: Linux 5.15.0-1005-raspi dwc2_hsotg
[    3.244977] kernel: usb usb1: SerialNumber: 3f980000.usb
[    3.245905] kernel: hub 1-0:1.0: USB hub found
[    3.246012] kernel: hub 1-0:1.0: 1 port detected
[    3.639772] kernel: usb 1-1: new high-speed USB device number 2 using dwc2
[    3.848142] kernel: usb 1-1: New USB device found, idVendor=0424, idProduct=9514, bcdDevice= 2.00
[    3.848173] kernel: usb 1-1: New USB device strings: Mfr=0, Product=0, SerialNumber=0
[    3.849346] kernel: hub 1-1:1.0: USB hub found
[    3.849498] kernel: hub 1-1:1.0: 5 ports detected
[    4.135790] kernel: usb 1-1.1: new high-speed USB device number 3 using dwc2
[    4.236287] kernel: usb 1-1.1: New USB device found, idVendor=0424, idProduct=ec00, bcdDevice= 2.00
[    4.236328] kernel: usb 1-1.1: New USB device strings: Mfr=0, Product=0, SerialNumber=0
[    4.239649] kernel: smsc95xx v2.0.0
[    4.371822] kernel: SMSC LAN8700 usb-001:003:01: attached PHY driver (mii_bus:phy_addr=usb-001:003:01, irq=POLL)
[    4.373170] kernel: smsc95xx 1-1.1:1.0 eth0: register 'smsc95xx' at usb-3f980000.usb-1.1, smsc95xx USB 2.0 Ethernet, b8:27:eb:9b:20:ee
[    4.390806] kernel: smsc95xx 1-1.1:1.0 enxb827eb9b20ee: renamed from eth0
[    4.959717] kernel: raid6: neonx8   gen()  1870 MB/s
[    5.027693] kernel: raid6: neonx8   xor()  1326 MB/s
[    5.095688] kernel: raid6: neonx4   gen()  1925 MB/s
[    5.163691] kernel: raid6: neonx4   xor()  1307 MB/s
[    5.231710] kernel: raid6: neonx2   gen()  1795 MB/s
[    5.299690] kernel: raid6: neonx2   xor()  1217 MB/s
[    5.367701] kernel: raid6: neonx1   gen()  1561 MB/s
[    5.435689] kernel: raid6: neonx1   xor()  1054 MB/s
[    5.467826] kernel: random: crng init done
[    5.503700] kernel: raid6: int64x8  gen()  1346 MB/s
[    5.571690] kernel: raid6: int64x8  xor()   764 MB/s
[    5.639691] kernel: raid6: int64x4  gen()  1542 MB/s
[    5.707699] kernel: raid6: int64x4  xor()   834 MB/s
[    5.775700] kernel: raid6: int64x2  gen()  1382 MB/s
[    5.843699] kernel: raid6: int64x2  xor()   726 MB/s
[    5.911700] kernel: raid6: int64x1  gen()  1020 MB/s
[    5.979697] kernel: raid6: int64x1  xor()   511 MB/s
[    5.979708] kernel: raid6: using algorithm neonx4 gen() 1925 MB/s
[    5.979717] kernel: raid6: .... xor() 1307 MB/s, rmw enabled
[    5.979725] kernel: raid6: using neon recovery algorithm
[    5.987443] kernel: xor: measuring software checksum speed
[    5.991761] kernel:    8regs           :  2341 MB/sec
[    5.995326] kernel:    32regs          :  2777 MB/sec
[    6.002844] kernel:    arm64_neon      :  1315 MB/sec
[    6.002855] kernel: xor: using function: 32regs (2777 MB/sec)
[    6.006824] kernel: async_tx: api initialized (async)
[    6.396287] kernel: Btrfs loaded, crc32c=crc32c-generic, zoned=yes, fsverity=no
[    6.866233] kernel: EXT4-fs (mmcblk0p2): mounted filesystem with ordered data mode. Opts: (null). Quota mode: none.
[    8.167978] systemd[1]: Inserted module 'autofs4'
[    8.284789] systemd[1]: systemd 249.11-0ubuntu3 running in system mode (+PAM +AUDIT +SELINUX +APPARMOR +IMA +SMACK +SECCOMP +GCRYPT +GNUTLS -OPENSSL +ACL +BLKID +CURL +ELFUTILS -FIDO2 +IDN2 -IDN +IPTC +KMOD +LIBCRYPTSETUP -LIBFDISK +PCRE2 -PWQUALITY -P11KIT -QRENCODE +BZIP2 +LZ4 +XZ +ZLIB +ZSTD -XKBCOMMON +UTMP +SYSVINIT default-hierarchy=unified)
[    8.287243] systemd[1]: Detected architecture arm64.
[    8.290122] systemd[1]: Hostname set to <ubuntu>.
[   10.207769] systemd[1]: Queued start job for default target Graphical Interface.
[   10.239457] systemd[1]: Created slice Slice /system/modprobe.
[   10.244765] systemd[1]: Created slice Slice /system/serial-getty.
[   10.249714] systemd[1]: Created slice Slice /system/systemd-fsck.
[   10.252993] systemd[1]: Created slice User and Session Slice.
[   10.253835] systemd[1]: Started Forward Password Requests to Wall Directory Watch.
[   10.255652] systemd[1]: Set up automount Arbitrary Executable File Formats File System Automount Point.
[   10.256402] systemd[1]: Reached target Slice Units.
[   10.256557] systemd[1]: Reached target Swaps.
[   10.256704] systemd[1]: Reached target Local Verity Protected Volumes.
[   10.257496] systemd[1]: Listening on Device-mapper event daemon FIFOs.
[   10.258556] systemd[1]: Listening on LVM2 poll daemon socket.
[   10.259999] systemd[1]: Listening on multipathd control socket.
[   10.290117] systemd[1]: Listening on RPCbind Server Activation Socket.
[   10.292033] systemd[1]: Listening on Syslog Socket.
[   10.293532] systemd[1]: Listening on fsck to fsckd communication Socket.
[   10.294348] systemd[1]: Listening on initctl Compatibility Named Pipe.
[   10.296966] systemd[1]: Listening on Journal Audit Socket.
[   10.298561] systemd[1]: Listening on Journal Socket (/dev/log).
[   10.301155] systemd[1]: Listening on Journal Socket.
[   10.303293] systemd[1]: Listening on Network Service Netlink Socket.
[   10.304907] systemd[1]: Listening on udev Control Socket.
[   10.306085] systemd[1]: Listening on udev Kernel Socket.
[   10.313436] systemd[1]: Mounting Huge Pages File System...
[   10.321570] systemd[1]: Mounting POSIX Message Queue File System...
[   10.329192] systemd[1]: Mounting NFSD configuration filesystem...
[   10.343339] systemd[1]: Mounting Kernel Debug File System...
[   10.353272] systemd[1]: Mounting Kernel Trace File System...
[   10.366497] systemd[1]: Starting Journal Service...
[   10.367321] systemd[1]: Condition check resulted in Kernel Module supporting RPCSEC_GSS being skipped.
[   10.379054] systemd[1]: Starting Set the console keyboard layout...
[   10.388892] systemd[1]: Starting Create List of Static Device Nodes...
[   10.401634] systemd[1]: Starting Monitoring of LVM2 mirrors, snapshots etc. using dmeventd or progress polling...
[   10.402497] systemd[1]: Condition check resulted in LXD - agent being skipped.
[   10.415821] systemd[1]: Starting Load Kernel Module configfs...
[   10.428871] systemd[1]: Starting Load Kernel Module drm...
[   10.439619] systemd[1]: Starting Load Kernel Module fuse...
[   10.440309] systemd[1]: Condition check resulted in OpenVSwitch configuration for cleanup being skipped.
[   10.453433] systemd[1]: Starting File System Check on Root Device...
[   10.554951] systemd[1]: Starting Load Kernel Modules...
[   10.563021] kernel: RPC: Registered named UNIX socket transport module.
[   10.563064] kernel: RPC: Registered udp transport module.
[   10.563073] kernel: RPC: Registered tcp transport module.
[   10.563081] kernel: RPC: Registered tcp NFSv4.1 backchannel transport module.
[   10.564444] systemd[1]: Starting Coldplug All udev Devices...
[   10.582666] systemd[1]: Mounted Huge Pages File System.
[   10.584423] systemd[1]: Mounted POSIX Message Queue File System.
[   10.585955] systemd[1]: Mounted Kernel Debug File System.
[   10.587426] systemd[1]: Mounted Kernel Trace File System.
[   10.592505] systemd[1]: Finished Create List of Static Device Nodes.
[   10.598923] systemd[1]: Finished Monitoring of LVM2 mirrors, snapshots etc. using dmeventd or progress polling.
[   10.604590] systemd[1]: modprobe@configfs.service: Deactivated successfully.
[   10.609729] systemd[1]: Finished Load Kernel Module configfs.
[   10.618518] systemd[1]: modprobe@fuse.service: Deactivated successfully.
[   10.637454] systemd[1]: Finished Load Kernel Module fuse.
[   10.647060] systemd[1]: Mounting FUSE Control File System...
[   10.655411] systemd[1]: Mounting Kernel Configuration File System...
[   10.667589] systemd[1]: Started File System Check Daemon to report status.
[   10.683250] systemd[1]: Mounted FUSE Control File System.
[   10.685725] systemd[1]: Mounted Kernel Configuration File System.
[   10.695992] systemd[1]: Finished Load Kernel Modules.
[   10.706424] systemd[1]: Starting Apply Kernel Variables...
[   10.765165] systemd[1]: modprobe@drm.service: Deactivated successfully.
[   10.772126] systemd[1]: Finished Load Kernel Module drm.
[   10.798601] systemd[1]: Started Journal Service.
[   10.875485] kernel: Installing knfsd (copyright (C) 1996 okir@monad.swb.de).
[   10.908574] kernel: EXT4-fs (mmcblk0p2): re-mounted. Opts: discard,errors=remount-ro. Quota mode: none.
[   11.616574] kernel: loop0: detected capacity change from 0 to 199768
[   11.625718] kernel: loop1: detected capacity change from 0 to 117656
[   11.649474] kernel: loop2: detected capacity change from 0 to 147080
[   11.676731] kernel: loop3: detected capacity change from 0 to 77328
[   11.691724] kernel: loop4: detected capacity change from 0 to 79224
[   11.692399] kernel: loop5: detected capacity change from 0 to 147080
[   12.723398] kernel: vc_sm_cma: module is from the staging directory, the quality is unknown, you have been warned.
[   12.725497] kernel: bcm2835_vc_sm_cma_probe: Videocore shared memory driver
[   12.725529] kernel: [vc_sm_connected_init]: start
[   12.735768] kernel: [vc_sm_connected_init]: installed successfully
[   12.787147] kernel: mc: Linux media interface: v0.10
[   12.799710] kernel: gpiomem-bcm2835 3f200000.gpiomem: Initialised: Registers at 0x3f200000
[   12.865439] kernel: videodev: Linux video capture interface: v2.00
[   12.896030] kernel: snd_bcm2835: module is from the staging directory, the quality is unknown, you have been warned.
[   12.932188] kernel: bcm2835_audio bcm2835_audio: card created with 8 channels
[   13.018725] kernel: bcm2835_mmal_vchiq: module is from the staging directory, the quality is unknown, you have been warned.
[   13.024369] kernel: bcm2835_mmal_vchiq: module is from the staging directory, the quality is unknown, you have been warned.
[   13.031112] kernel: bcm2835_mmal_vchiq: module is from the staging directory, the quality is unknown, you have been warned.
[   13.056081] kernel: bcm2835_isp: module is from the staging directory, the quality is unknown, you have been warned.
[   13.068599] kernel: bcm2835_v4l2: module is from the staging directory, the quality is unknown, you have been warned.
[   13.080071] kernel: bcm2835-isp bcm2835-isp: Device node output[0] registered as /dev/video13
[   13.080431] kernel: bcm2835_codec: module is from the staging directory, the quality is unknown, you have been warned.
[   13.080522] kernel: bcm2835-isp bcm2835-isp: Device node capture[0] registered as /dev/video14
[   13.080878] kernel: bcm2835-isp bcm2835-isp: Device node capture[1] registered as /dev/video15
[   13.081235] kernel: bcm2835-isp bcm2835-isp: Device node stats[2] registered as /dev/video16
[   13.081273] kernel: bcm2835-isp bcm2835-isp: Register output node 0 with media controller
[   13.081304] kernel: bcm2835-isp bcm2835-isp: Register capture node 1 with media controller
[   13.081320] kernel: bcm2835-isp bcm2835-isp: Register capture node 2 with media controller
[   13.081335] kernel: bcm2835-isp bcm2835-isp: Register capture node 3 with media controller
[   13.086237] kernel: bcm2835-isp bcm2835-isp: Device node output[0] registered as /dev/video20
[   13.087211] kernel: bcm2835-isp bcm2835-isp: Device node capture[0] registered as /dev/video21
[   13.088052] kernel: bcm2835-isp bcm2835-isp: Device node capture[1] registered as /dev/video22
[   13.088569] kernel: bcm2835-isp bcm2835-isp: Device node stats[2] registered as /dev/video23
[   13.088612] kernel: bcm2835-isp bcm2835-isp: Register output node 0 with media controller
[   13.088637] kernel: bcm2835-isp bcm2835-isp: Register capture node 1 with media controller
[   13.088669] kernel: bcm2835-isp bcm2835-isp: Register capture node 2 with media controller
[   13.088703] kernel: bcm2835-isp bcm2835-isp: Register capture node 3 with media controller
[   13.088972] kernel: bcm2835-isp bcm2835-isp: Loaded V4L2 bcm2835-isp
[   13.097772] kernel: bcm2835-codec bcm2835-codec: Device registered as /dev/video10
[   13.097837] kernel: bcm2835-codec bcm2835-codec: Loaded V4L2 decode
[   13.110500] kernel: bcm2835-codec bcm2835-codec: Device registered as /dev/video11
[   13.110569] kernel: bcm2835-codec bcm2835-codec: Loaded V4L2 encode
[   13.117968] kernel: bcm2835-codec bcm2835-codec: Device registered as /dev/video12
[   13.118040] kernel: bcm2835-codec bcm2835-codec: Loaded V4L2 isp
[   13.120323] kernel: bcm2835-codec bcm2835-codec: Device registered as /dev/video18
[   13.120373] kernel: bcm2835-codec bcm2835-codec: Loaded V4L2 image_fx
[   13.128729] kernel: bcm2835-codec bcm2835-codec: Device registered as /dev/video31
[   13.128794] kernel: bcm2835-codec bcm2835-codec: Loaded V4L2 encode_image
[   13.149639] kernel: smsc95xx 1-1.1:1.0 eth0: renamed from enxb827eb9b20ee
[   13.378632] kernel: cfg80211: Loading compiled-in X.509 certificates for regulatory database
[   13.387204] kernel: cfg80211: Loaded X.509 cert 'sforshee: 00b28ddf47aef9cea7'
[   13.571133] kernel: brcmfmac: F1 signature read @0x18000000=0x1541a9a6
[   13.589633] kernel: brcmfmac: brcmf_fw_alloc_request: using brcm/brcmfmac43430-sdio for chip BCM43430/1
[   13.590966] kernel: usbcore: registered new interface driver brcmfmac
[   13.655894] kernel: brcmfmac mmc1:0001:1: Direct firmware load for brcm/brcmfmac43430-sdio.raspberrypi,3-model-b.bin failed with error -2
[   13.919710] kernel: brcmfmac: brcmf_fw_alloc_request: using brcm/brcmfmac43430-sdio for chip BCM43430/1
[   13.919910] kernel: brcmfmac: brcmf_fw_alloc_request: using brcm/brcmfmac43430-sdio for chip BCM43430/1
[   13.929096] kernel: brcmfmac: brcmf_c_preinit_dcmds: Firmware: BCM43430/1 wl0: Jul 19 2021 03:24:18 version 7.45.98 (TOB) (56df937 CY) FWID 01-8e14b897
[   15.298901] kernel: audit: type=1400 audit(1650616980.611:2): apparmor="STATUS" operation="profile_load" profile="unconfined" name="nvidia_modprobe" pid=603 comm="apparmor_parser"
[   15.298972] kernel: audit: type=1400 audit(1650616980.611:3): apparmor="STATUS" operation="profile_load" profile="unconfined" name="nvidia_modprobe//kmod" pid=603 comm="apparmor_parser"
[   15.301881] kernel: audit: type=1400 audit(1650616980.615:4): apparmor="STATUS" operation="profile_load" profile="unconfined" name="/usr/bin/man" pid=605 comm="apparmor_parser"
[   15.301930] kernel: audit: type=1400 audit(1650616980.615:5): apparmor="STATUS" operation="profile_load" profile="unconfined" name="man_filter" pid=605 comm="apparmor_parser"
[   15.301958] kernel: audit: type=1400 audit(1650616980.615:6): apparmor="STATUS" operation="profile_load" profile="unconfined" name="man_groff" pid=605 comm="apparmor_parser"
[   15.302141] kernel: audit: type=1400 audit(1650616980.615:7): apparmor="STATUS" operation="profile_load" profile="unconfined" name="lsb_release" pid=602 comm="apparmor_parser"
[   15.361342] kernel: audit: type=1400 audit(1650616980.675:8): apparmor="STATUS" operation="profile_load" profile="unconfined" name="tcpdump" pid=606 comm="apparmor_parser"
[   15.374437] kernel: audit: type=1400 audit(1650616980.687:9): apparmor="STATUS" operation="profile_load" profile="unconfined" name="/usr/lib/snapd/snap-confine" pid=607 comm="apparmor_parser"
[   15.375316] kernel: audit: type=1400 audit(1650616980.687:10): apparmor="STATUS" operation="profile_load" profile="unconfined" name="/usr/lib/snapd/snap-confine//mount-namespace-capture-helper" pid=607 comm="apparmor_parser"
[   15.394927] kernel: audit: type=1400 audit(1650616980.707:11): apparmor="STATUS" operation="profile_load" profile="unconfined" name="/usr/lib/NetworkManager/nm-dhcp-client.action" pid=604 comm="apparmor_parser"
[   20.439911] kernel: smsc95xx 1-1.1:1.0 eth0: hardware isn't capable of remote wakeup
[   20.573243] kernel: smsc95xx 1-1.1:1.0 eth0: Link is Down
[   23.713396] kernel: smsc95xx 1-1.1:1.0 eth0: Link is Up - 100Mbps/Full - flow control off
[   23.713487] kernel: IPv6: ADDRCONF(NETDEV_CHANGE): eth0: link becomes ready
[   25.478117] kernel: uart-pl011 3f201000.serial: no DMA platform data
[   27.909169] kernel: brcmfmac: brcmf_cfg80211_set_power_mgmt: power save enabled
[   28.884963] kernel: loop6: detected capacity change from 0 to 8
[   29.971506] kernel: NFSD: Using nfsdcld client tracking operations.
[   29.971534] kernel: NFSD: no clients to reclaim, skipping NFSv4 grace period (net f00005c9)
